Instructions on how to wire up a parallel-port cable 
suitable for the parallel-port PIPX driver, PIPX.


< This cable works perfectly with Quake and Duke Nukem 3D >


Pin Configuration

1-
2-15
3-13
4-12
5-10
6-11
7-
8-18
9-
10-5
11-6
12-4
13-3
14-
15-2
16-
17-
18-
19-19
20-20
21-21
22-22
23-23
24-24
25-25

* If the number is blank..its not used.
** Also add another line....Shield to shield for ground.
